### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:14.7 (WebPack) - P.20131013 | Target Family: | Spartan3
OS Platform: | NT64 | Target Device: | xc3s1000
Project ID (random number) | 9420f6f36f0143a08d15315a9cec1ff2.1BF1B53EA1BD4DB3BFDAA978FAEA3C01.1 | Target Package: | ft256
Registration ID | 210945993_0_0_712 | Target Speed: | -5
Date Generated | 2014-12-17T15:32:58 | Tool Flow | ISE

User Environment
OS Name | Microsoft , 64-bit | OS Release | major release (build 9200)
CPU Name | Intel(R) Core(TM) i7-3540M CPU @ 3.00GHz | CPU Speed | 2990 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
Adders/Subtractors=1 19-bit adder=1 Comparators=8 10-bit comparator greatequal=2 10-bit comparator less=5 11-bit comparator less=1 Counters=2 10-bit up counter=2 Latches=1 19-bit latch=1 Registers=1 Flip-Flops=1 | MiscellaneousStatistics AGG_BONDED_IO=27 AGG_IO=27 AGG_SLICE=19 NUM_4_INPUT_LUT=35 NUM_BONDED_IOB=27 NUM_BUFGMUX=2 NUM_CYMUX=18 NUM_SLICEL=19 NUM_SLICE_FF=21 NUM_XOR=20 | NetStatistics NumNets_Active=71 NumNets_Gnd=1 NumNets_Vcc=1 NumNodesOfType_Active_CLKPIN=11 NumNodesOfType_Active_CNTRLPIN=6 NumNodesOfType_Active_DOUBLE=33 NumNodesOfType_Active_DUMMY=96 NumNodesOfType_Active_DUMMYESC=1 NumNodesOfType_Active_GLOBAL=12 NumNodesOfType_Active_HUNIHEX=4 NumNodesOfType_Active_INPUT=110 NumNodesOfType_Active_IOBOUTPUT=1 NumNodesOfType_Active_OMUX=42 NumNodesOfType_Active_OUTPUT=43 NumNodesOfType_Active_PREBXBY=22 NumNodesOfType_Active_VFULLHEX=3 NumNodesOfType_Active_VUNIHEX=1 NumNodesOfType_Vcc_CNTRLPIN=2 NumNodesOfType_Vcc_INPUT=1 NumNodesOfType_Vcc_PREBXBY=1 NumNodesOfType_Vcc_VCCOUT=2 SiteStatistics IOB-DIFFM=11 IOB-DIFFS=11 SLICEL-SLICEM=9 | SiteSummary BUFGMUX=2 BUFGMUX_GCLKMUX=2 BUFGMUX_GCLK_BUFFER=2 IOB=27 IOB_INBUF=1 IOB_OUTBUF=26 IOB_PAD=27 SLICEL=19 SLICEL_CYMUXF=10 SLICEL_CYMUXG=8 SLICEL_F=18 SLICEL_F5MUX=3 SLICEL_FFX=10 SLICEL_FFY=11 SLICEL_G=17 SLICEL_GNDF=10 SLICEL_GNDG=8 SLICEL_XORF=10 SLICEL_XORG=10

Configuration Data
BUFGMUX S=[S_INV:2] [S:0] BUFGMUX_GCLKMUX DISABLE_ATTR=[LOW:2] S=[S_INV:2] [S:0] IOB O1=[O1_INV:0] [O1:26] IOB_OUTBUF IN=[IN_INV:0] [IN:26] IOB_PAD DRIVEATTRBOX=[12:26] IOATTRBOX=[LVCMOS25:27] SLEW=[SLOW:26] | SLICEL BX=[BX_INV:0] [BX:5] BY=[BY:1] [BY_INV:0] CE=[CE:5] [CE_INV:0] CIN=[CIN_INV:0] [CIN:8] CLK=[CLK:11] [CLK_INV:0] SR=[SR:1] [SR_INV:0] SLICEL_CYMUXF 0=[0:10] [0_INV:0] 1=[1_INV:0] [1:10] | SLICEL_CYMUXG 0=[0:8] [0_INV:0] SLICEL_F5MUX S0=[S0:3] [S0_INV:0] SLICEL_FFX CE=[CE:5] [CE_INV:0] CK=[CK:10] [CK_INV:0] D=[D:10] [D_INV:0] FFX_INIT_ATTR=[INIT0:10] FFX_SR_ATTR=[SRLOW:10] LATCH_OR_FF=[FF:10] SYNC_ATTR=[ASYNC:10] | SLICEL_FFY CE=[CE:5] [CE_INV:0] CK=[CK:11] [CK_INV:0] D=[D:11] [D_INV:0] FFY_INIT_ATTR=[INIT0:11] FFY_SR_ATTR=[SRLOW:11] LATCH_OR_FF=[FF:11] SR=[SR:1] [SR_INV:0] SYNC_ATTR=[ASYNC:10] [SYNC:1] | SLICEL_XORF 1=[1_INV:0] [1:10]

Pin Data
BUFGMUX I0=2 O=2 S=2 BUFGMUX_GCLKMUX I0=2 OUT=2 S=2 BUFGMUX_GCLK_BUFFER IN=2 OUT=2 IOB I=1 O1=26 PAD=27 IOB_INBUF IN=1 OUT=1 IOB_OUTBUF IN=26 OUT=26 IOB_PAD PAD=27 SLICEL BX=5 BY=1 CE=5 CIN=8 CLK=11 COUT=8 F1=15 F2=15 F3=6 F4=6 G1=17 G2=17 G3=9 G4=8 SR=1 X=8 XQ=10 Y=4 YQ=11 | SLICEL_CYMUXF 0=10 1=10 OUT=10 S0=10 SLICEL_CYMUXG 0=8 1=8 OUT=8 S0=8 SLICEL_F A1=15 A2=15 A3=6 A4=6 D=18 SLICEL_F5MUX F=3 G=3 OUT=3 S0=3 SLICEL_FFX CE=5 CK=10 D=10 Q=10 | SLICEL_FFY CE=5 CK=11 D=11 Q=11 SR=1 SLICEL_G A1=17 A2=17 A3=9 A4=8 D=17 SLICEL_GNDF 0=10 SLICEL_GNDG 0=8 SLICEL_XORF 0=10 1=10 O=10 SLICEL_XORG 0=10 1=10 O=10 |

Tool Usage
Command Line History xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -i -p xc3s1000-ft256-5 <fname>.ngc <fname>.ngd map -intstyle ise -p xc3s1000-ft256-5 -cm area -ir off -pr off -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf par -w -intstyle ise -ol high -t 1 <fname>.ncd <fname>.ncd <fname>.pcf trce -intstyle ise -v 3 -s 5 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf bitgen -intstyle ise -f <fname>.ut <fname>.ncd

Software Quality
Run Statistics
Program Name | Runs Started | Runs Finished | Errors | Fatal Errors | Internal Errors | Exceptions | Core Dumps
_impact | 37 | 24 | 0 | 0 | 0 | 0 | 0
bitgen | 28 | 28 | 0 | 0 | 0 | 0 | 0
map | 34 | 32 | 0 | 0 | 0 | 0 | 0
ngdbuild | 36 | 36 | 0 | 0 | 0 | 0 | 0
par | 32 | 30 | 2 | 0 | 0 | 0 | 0
trce | 30 | 30 | 0 | 0 | 0 | 0 | 0
xst | 91 | 89 | 0 | 0 | 0 | 0 | 0

Project Statistics
PROP_Enable_Message_Filtering=false | PROP_FitterReportFormat=HTML
PROP_LastAppliedGoal=Balanced | PROP_LastAppliedStrategy=Xilinx Default (unlocked)
PROP_ManualCompileOrderImp=false | PROP_PropSpecInProjFile=Store all values
PROP_Simulator=Modelsim-SE Verilog | PROP_SynthTopFile=changed
PROP_Top_Level_Module_Type=HDL | PROP_UseSmartGuide=false
PROP_UserConstraintEditorPreference=Text Editor | PROP_intProjectCreationTimestamp=2014-12-16T17:16:04
PROP_intWbtProjectID=1BF1B53EA1BD4DB3BFDAA978FAEA3C01 | PROP_intWbtProjectIteration=1
PROP_intWorkingDirLocWRTProjDir=Same | PROP_intWorkingDirUsed=No
PROP_AutoTop=false | PROP_DevFamily=Spartan3
PROP_DevDevice=xc3s1000 | PROP_DevFamilyPMName=spartan3
PROP_DevPackage=ft256 | PROP_Synthesis_Tool=XST (VHDL/Verilog)
PROP_DevSpeed=-5 | PROP_PreferredLanguage=Verilog
FILE_UCF=1 | FILE_VERILOG=4

Unisim Statistics
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_BUFG=1 | NGDBUILD_NUM_BUFGP=1 | NGDBUILD_NUM_FDC=10 | NGDBUILD_NUM_FDCE=10
NGDBUILD_NUM_FDR=1 | NGDBUILD_NUM_GND=1 | NGDBUILD_NUM_LUT2=17 | NGDBUILD_NUM_LUT3_D=1
NGDBUILD_NUM_LUT4=12 | NGDBUILD_NUM_LUT4_D=2 | NGDBUILD_NUM_MUXCY=18 | NGDBUILD_NUM_MUXF5=3
NGDBUILD_NUM_OBUF=26 | NGDBUILD_NUM_VCC=1 | NGDBUILD_NUM_XORCY=20
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_BUFG=2 | NGDBUILD_NUM_FDC=10 | NGDBUILD_NUM_FDCE=10 | NGDBUILD_NUM_FDR=1
NGDBUILD_NUM_GND=1 | NGDBUILD_NUM_IBUFG=1 | NGDBUILD_NUM_LUT2=17 | NGDBUILD_NUM_LUT3_D=1
NGDBUILD_NUM_LUT4=12 | NGDBUILD_NUM_LUT4_D=2 | NGDBUILD_NUM_MUXCY=18 | NGDBUILD_NUM_MUXF5=3
NGDBUILD_NUM_OBUF=26 | NGDBUILD_NUM_VCC=1 | NGDBUILD_NUM_XORCY=20

XST Command Line Options
XST_OPTION_SUMMARY
-ifn=<fname>.prj | -ifmt=mixed | -ofn=<design_top> | -ofmt=NGC
-p=xc3s1000-5-ft256 | -top=<design_top> | -opt_mode=Speed | -opt_level=1
-iuc=NO | -keep_hierarchy=No | -netlist_hierarchy=As_Optimized | -rtlview=Yes
-glob_opt=AllClockNets | -read_cores=YES | -write_timing_constraints=NO | -cross_clock_analysis=NO
-bus_delimiter=<> | -slice_utilization_ratio=100 | -bram_utilization_ratio=100 | -verilog2001=YES
-fsm_extract=YES | -fsm_encoding=Auto | -safe_implementation=No | -fsm_style=LUT
-ram_extract=Yes | -ram_style=Auto | -rom_extract=Yes | -shreg_extract=YES
-rom_style=Auto | -auto_bram_packing=NO | -resource_sharing=YES | -async_to_sync=NO
-mult_style=Auto | -iobuf=YES | -max_fanout=500 | -bufg=8
-register_duplication=YES | -register_balancing=No | -optimize_primitives=NO | -use_clock_enable=Yes
-use_sync_set=Yes | -use_sync_reset=Yes | -iob=Auto | -equivalent_register_removal=YES
-slice_utilization_ratio_maxmargin=5